root@UltraLite-AVB:/opt# dmesg
[    0.000000] Linux version 2.6.32-rc8 (jenkins@mac-mini-slave1) (gcc version 4.5.1 (Sourcery G++ Lite 2010.09-50) ) #1 PREEMPT Wed Jul 3 11:23:44 EDT 2019
[    0.000000] CPU: ARM926EJ-S [41069265] revision 5 (ARMv5TEJ), cr=00053177
[    0.000000] CPU: VIVT data cache, VIVT instruction cache
[    0.000000] Machine: DaVinci DA850/OMAP-L138 EVM
[    0.000000] ss_early_mac
[    0.000000] ss_early_phy
[    0.000000] Memory policy: ECC disabled, Data cache writeback
[    0.000000] On node 0 totalpages: 14080
[    0.000000] free_area_init_node: node 0, pgdat c03ce7b0, node_mem_map c041f000
[    0.000000]   DMA zone: 110 pages used for memmap
[    0.000000]   DMA zone: 0 pages reserved
[    0.000000]   DMA zone: 13970 pages, LIFO batch:3
[    0.000000] DaVinci da850/omap-l138/am18x variant 0x1
[    0.000000] Built 1 zonelists in Zone order, mobility grouping on.  Total pages: 13970
[    0.000000] Kernel command line: mem=55M console=ttyS0,115200n8 root=/dev/ram0 rw initrd=0xc1180000,16M lpj=1138688 mac=00:01:f2:01:2a:7a phy_id=1 mtdparts=s25fl256s:5832704(Boot),6225920(Linux),8388608(RootFs),-(User_Data) ver_ssuboot=Jul-03-2019-e7987b4
[    0.000000] PID hash table entries: 256 (order: -2, 1024 bytes)
[    0.000000] Dentry cache hash table entries: 8192 (order: 3, 32768 bytes)
[    0.000000] Inode-cache hash table entries: 4096 (order: 2, 16384 bytes)
[    0.000000] Memory: 55MB = 55MB total
[    0.000000] Memory: 35148KB available (3584K code, 444K data, 152K init, 0K highmem)
[    0.000000] SLUB: Genslabs=11, HWalign=32, Order=0-3, MinObjects=0, CPUs=1, Nodes=1
[    0.000000] Hierarchical RCU implementation.
[    0.000000] NR_IRQS:245
[    0.000000] Console: colour dummy device 80x30
[    0.000353] Calibrating delay loop (skipped) preset value.. 569.34 BogoMIPS (lpj=1138688)
[    0.000584] Mount-cache hash table entries: 512
[    0.001573] CPU: Testing write buffer coherency: ok
[    0.007976] DaVinci: 144 gpio irqs
[    0.010033] NET: Registered protocol family 16
[    0.099464]
[    0.099483] EMIF Pinmux Setup
[    0.099495]
[    0.153760] bio: create slab <bio-0> at 0
[    0.161056] SCSI subsystem initialized
[    0.163394] Generic PHY: Registered new driver
[    0.172775] Switching to clocksource timer0_1
[    0.194627] musb_hdrc: version 6.0, cppi4.1-dma, peripheral, debug=0
[    0.196428] NET: Registered protocol family 2
[    0.196780] IP route cache hash table entries: 1024 (order: 0, 4096 bytes)
[    0.197845] TCP established hash table entries: 2048 (order: 2, 16384 bytes)
[    0.197992] TCP bind hash table entries: 2048 (order: 1, 8192 bytes)
[    0.198089] TCP: Hash tables configured (established 2048 bind 2048)
[    0.198120] TCP reno registered
[    0.198501] NET: Registered protocol family 1
[    0.199450] RPC: Registered udp transport module.
[    0.199497] RPC: Registered tcp transport module.
[    0.199526] RPC: Registered tcp NFSv4.1 backchannel transport module.
[    0.200178] Trying to unpack rootfs image as initramfs...
[    0.203266] rootfs image is not initramfs (no cpio magic); looks like an initrd
[    0.446688] Freeing initrd memory: 16384K
[    0.449784]
[    0.449805] init da850_evm_config_ssmac
[    0.449819]
[    0.450717]
[    0.450739] init da850_evm_config_emac
[    0.450751]
[    0.450788] EMAC: RMII PHY configured, MII PHY will not be functional
[    0.526524] squashfs: version 4.0 (2009/01/31) Phillip Lougher
[    0.535934] JFFS2 version 2.2. (NAND) (SUMMARY)  © 2001-2006 Red Hat, Inc.
[    0.540233] msgmni has been set to 100
[    0.542072] io scheduler noop registered
[    0.542123] io scheduler anticipatory registered (default)
[    0.637740]
[    0.637762]
[    0.637772] SSLCD_init_module
[    0.637784]
[    0.637848]
[    0.637860]
[    0.637868] ss gpio init - debug mode is disabled
[    0.637916] ss gpio: registered module successfully
[    0.637968] GPIO Hook
[    0.638458] Serial: 8250/16550 driver, 3 ports, IRQ sharing disabled
[    0.639508] kStart Tasklet: USB_TBT Ctrl Pkt
[    0.639787] kStart Tasklet: USB Bulk Pkt
[    0.641393] kStart Tasklet: LPD
[    0.641669] kStart Tasklet: USB Vbus Rst
[    0.645735] serial8250.0: ttyS0 at MMIO 0x1c42000 (irq = 25) is a 16550A
[    0.994906] console [ttyS0] enabled
[    1.001082] serial8250.0: ttyS1 at MMIO 0x1d0c000 (irq = 53) is a 16550A
[    1.010453] serial8250.0: ttyS2 at MMIO 0x1d0d000 (irq = 61) is a 16550A
[    1.021965] brd: module loaded
[    1.035116] m25p80 spi1.0: found mx25l25645g, expected s25fl256s
[    1.041632] 4 cmdlinepart partitions found on MTD device s25fl256s
[    1.048046] Creating 4 MTD partitions on "s25fl256s":
[    1.053268] 0x000000000000-0x000000590000 : "Boot"
[    1.063130] 0x000000590000-0x000000b80000 : "Linux"
[    1.072011] 0x000000b80000-0x000001380000 : "RootFs"
[    1.080736] 0x000001380000-0x000002000000 : "User_Data"
[    1.090130] spi_davinci spi_davinci.1: Controller at 0xfef0e000
[    1.099096] spi_davinci spi_davinci.0: Controller at 0xfec41000
[    1.109907] SMSC LAN83C185: Registered new driver
[    1.115715] SMSC LAN8187: Registered new driver
[    1.121463] SMSC LAN8700: Registered new driver
[    1.127004] SMSC LAN911x Internal PHY: Registered new driver
[    1.133786] SMSC LAN8710/LAN8720: Registered new driver
[    1.139324] console [netcon0] enabled
[    1.143132] netconsole: network logging started
[    1.148654] i2c /dev entries driver
[    1.155362] watchdog watchdog: heartbeat 60 sec
[    1.163697] cpuidle: using governor ladder
[    1.171303] cpuidle: using governor menu
[    1.177520] Advanced Linux Sound Architecture Driver Version 1.0.21.
[    1.186410] ALSA device list:
[    1.189571]   No soundcards found.
[    1.193103] oprofile: using timer interrupt.
[    1.199232] TCP cubic registered
[    1.202745] NET: Registered protocol family 17
[    1.210759] registered taskstats version 1
[    1.215452] ssmac_probe (tamio)
[    1.215476]
[    1.220417] iobase: C3880000, size: 00040000
[    1.220440]
[    1.228124] ssmac_hard_reset
[    1.231275] [0x2828] = 0000018F
[    1.234557] [0x2828] = 0000019F
[    1.237807] reset_error_counters
[    1.241958] davinci_emac_init
[    1.241981]
[    1.246809]
[    1.246830] davinci_emac_probe
[    1.246842]
[    1.253051] emac_bus_frequency: 114000000
[    1.257225] DaVinci mac address 00:00:00:00:00:00
[    1.262123] davinci_emac_probe: using random MAC addr: 92:49:ba:1e:55:ba
[    1.270962] mdiobus_register
[    1.274945] mdiobus_scan error addr 00
[    1.279068] phy_device_create addr 01, id 7C0F1
[    1.284699] phy_device_register OK addr: 01
[    1.289190] mdiobus_scan error addr 04
[    1.293169] mdiobus_scan error addr 1F
[    1.297035] emac-mii: probed
[    1.299953] emac-mii: probed
[    1.304304] RAMDISK: gzip image found at block 0
[    3.870570] VFS: Mounted root (ext2 filesystem) on device 1:0.
[    3.877046] Freeing init memory: 152K
[    7.230264] ssmac_open
[    7.247322] ssmac - phy_connect
[    7.262259] ssmac PHY driver name: SMSC LAN8710/LAN8720, ssmac PHY ID: 0x07c0f1
[    7.305924] ssmac PHY dflt No Link Speed: 100
[    7.310505] ssmac_firm_reset - 1000
[    9.261423] Link Off
[    9.263667] ssmac_firm_reset - 100
[    9.267119] PHY Name: 1:01 - PHY ID: 0x7c0f1 - Link is Down
[    9.272557]  - 10/Half
[    9.274945]
[   15.061144] ssmac_avb_open: successful
[   16.269216] SysLink version : 2.21.02.10
[   16.269243] SysLink module created on Date:Mar  8 2016 Time:12:51:06
[   16.281914] Trace enabled
[   16.285882] Trace SetFailureReason enabled
[   17.838117]
[   17.838142] ss_gpio: Wait for LPD
[   17.838155]
[  811.309294] ssmac_firm_reset - 100
[  811.312753] Link On
[  811.314918] PHY Name: 1:01 - PHY ID: 0x7c0f1 - Link is Up
[  811.320187]  - 100/Full
[  811.322663]
root@UltraLite-AVB:/opt#
